nailing studs

pipe penetrations

fire-rated penetrations

through-wall penetrations

undulating facades

shaft liners

fire-rated shafts

screws at 12” o.c.

latex caulk and backer rod

column erection

hand blown fixtures

reclaimed hardwood

exposed beams

drilling the pole

driving piles

countersinking the head

exposed conduit

concrete vibrators

wood trusses

hot-mopped asphalt

steel erection

dampproofing

pulling wire

gluing it up

gang nailed

king studs

double headers

hose bibs

rod anchors

gutter flashing

deep grinding

stuffing boxes

furring strips

dry stacking

she bolts

sex bolts

backfill

taking a core sample

butt joints

butt glazing

exposed membrane

deep datum penetration

sack rub finish

oil-rubbed brass

hot-rolled steel

groin vaults

angles of repose

blown insulation

loss of skin friction

removable mullions

standing seams

spread footings

loading docks

recessed cans

concealed openings

beds of caulk

defenestration

ganged vent stacks

drip edges

means of egress

consolidated fill

knuckle joints

slab penetrations

radius of gyration

tongue and groove joints

slenderness ratio